|  |  |  |
| --- | --- | --- |
|  | **NEMA 17 Stepper Motor** | **28BYJ-48 Stepper Motor** |
| **Rated Voltage** | 9-12 V | 5 V |
| **Rated Current** | 1.4 A |  |
| **Step Angle** | 0.9 degrees per step (micro stepping available) | 5.6 degrees per step |
| **Torque** | >= 0.127 Nm | >0.00343 Nm |
| **Price** | ~£10 | ~£8 |
| **Driver Included** | No | Yes (ULN2003A) |
| **Driver Price (if, not included)** | ~£3-5 | N/A |
| **Weight** | 200 g | 33 g |
| **Dimensions** | 42.3 x 42.3 x 26.5 mm | 40 x 30 x 19 mm |